**PSDK Version 21:**

Fix main window widgets display problem in languages besides Chinese.

**Gimbal Version 12:**

Gimbal will calibrate faster and fix the problem that calibrating incorrectly sometimes.

**GL60 Plus update method:**

1. Prepare a 4~32G TF memory card and a card reader, insert the TF card into the card reader, and then insert the card reader into the USB port of the computer;
2. Put the zip package into the TF card and directory first;
3. Then unzip it directly to the current folder;
4. Place the folder "GL60\_Plus" in the root directory of the TF card, which contains the firmware to be upgraded.
5. Eject the TF card, unplug the card reader and pull out the TF card;
6. Insert the TF card into the TF card slot under the GL60 Plus light body;
7. Hook up the GL60 Plus to the drone and turn it on;
8. Wait until the program upgrade is complete and the GL60 Plus starts automatically;
9. Remove the TF card to finish the upgrade.