**PSDK Version 21:**

Adapt latest M300 firmware;

**GL60 Plus update method:**

1. Prepare a 4~32G TF memory card and a card reader, insert the TF card into the card reader, and then insert the card reader into the USB port of the computer;
2. Put the zip package into the TF card and directory first;
3. Then unzip it directly to the current folder;
4. Place the folder "GimbalLight300W" in the root directory of the TF card, which contains the firmware to be upgraded.
5. Eject the TF card, unplug the card reader and pull out the TF card;
6. Insert the TF card into the TF card slot under the GL300 Plus light body;
7. Hook up the GL300 to the drone and turn it on;
8. Wait until the program upgrade is complete and the GL300 starts automatically;
9. Remove the TF card to finish the upgrade.