**PSDK Version 22:**

Firmware to adapt M350.

**IR10 update method:**

1. Prepare a 4~32G TF memory card and a card reader, insert the TF card into the card reader, and then insert the card reader into the USB port of the computer;
2. Put the zip package into the TF card and directory first;
3. Then unzip it directly to the current folder;
4. Place the folder " InfraredLaser" in the root directory of the TF card, which contains the firmware to be upgraded.
5. Eject the TF card, unplug the card reader and pull out the TF card;
6. Insert the TF card into the TF card slot on the IR10 light body;
7. Hook up the IR10 to the drone and turn it on;
8. Wait until the program upgrade is complete and the IR10 starts automatically;
9. Remove the TF card to finish the upgrade.