**MP130 V2 firmware version- 02.01.04.45：**

**New Features:**

1. Based on PSDK330 adapted to DJI M300 drone firmware version V5
2. Add recording broadcast control, Text-to-speech control, volume adjustment control on DJI Pilot.
3. Add floating window with volume display, firmware version number display, SN code display on DJI Pilot
4. Add TTS language selection and speed selection save function.
5. Add English firmware version voice broadcast.

**Fixed issues:**

1. Fix the problem that the volume of the icon control is not synchronized with the volume of the floating window.
2. Fix other known issues.

**Current Issues：**

1. MP130 V2 floating window plays background sound, click to switch the loop mode, it will start the background sound playback, you can click the play/stop button to turn it off.

**Cautions：**

1. MP130S/MP130V2 does not support DJI Assistant software firmware upgrade at this time
2. To upgrade the MP130S/MP130V2, you need to prepare a TF/SD card and copy the firmware to the TF/SD card.